
#------------------------------------------------------------------------------
# URL: 		https://de.wikipedia.org/wiki/Aria_(Software)
# Reference:	https://github.com/aria2/aria2/blob/master/doc/manual-src/en/technical-notes.rst
# From:		Joerg Jenderek
# Note:		only version 1 suited
# check for valid version one
0		beshort		0x0001
# skip most uncompressed DEGAS med-res bitmap *.PI2 and GEM bitmap (v1) *.IMG
# by test for valid infoHashCheck extension
>2		ubelong&0xffFFffFE	0x00000000
# skip DEGAS med-res bitmap DIAGRAM1.PI2 by test for valid length of download
>>(6.L+14)	ubequad			>0
>>>0	use     aria
0	name	aria
# version; (0x0000) or (0x0001); for 0 all multi-byte are in host byte order. For 1 big endian
>0	beshort		x	aria2 control file, version %u
#!:mime	application/octet-stream
!:mime	application/x-aria
!:ext	aria2
# EXTension; if EXT[3]&1 == 1 checks whether saved InfoHash and current downloading the same; infoHashCheck extension
>2		ubelong		!0	\b, infoHashCheck %#x
# info hash length like: 0 14h
>6		ubelong		!0	\b, %#x bytes info hash
# info hash; BitTorrent InfoHash
>>10		ubequad		x	%#16.16llx...
# piece length; the length of the piece like: 400h 100000h
>(6.L+10)	ubelong		x	\b, piece length 0x%x
# total length; the total length of the download
>(6.L+14)	ubequad		x	\b, total length %llu
#>(6.L+14)	ubequad		x	\b, total length %#llx
# upload length; the uploaded length of download like: 0 400h
>(6.L+22)	ubequad		!0	\b, upload length %#llx
# bitfield length; the length of bitfield like: 4 6 Ah 10h 13h 167h
>(6.L+30)	ubelong		x	\b, %#x bytes bitfield
# bitfield; bitfield which represents current download progress
>(6.L+34)	ubequad		!0	%#llx...

