
#------------------------------------------------------------------------------
# $File: sun,v 1.28 2019/04/19 00:42:27 christos Exp $
# sun:  file(1) magic for Sun machines
#
# Values for big-endian Sun (MC680x0, SPARC) binaries on pre-5.x
# releases.  (5.x uses ELF.)  Entries for executables without an
# architecture type, used before the 68020-based Sun-3's came out,
# are in aout, as they're indistinguishable from other big-endian
# 32-bit a.out files.
#
0	belong&077777777	0600413		a.out SunOS SPARC demand paged
>0	byte		&0x80
>>20	belong		<4096		shared library
>>20	belong		=4096		dynamically linked executable
>>20	belong		>4096		dynamically linked executable
>0	byte		^0x80		executable
>16	belong		>0		not stripped

0	belong&077777777	0600410		a.out SunOS SPARC pure
>0	byte		&0x80		dynamically linked executable
>0	byte		^0x80		executable
>16	belong		>0		not stripped

0	belong&077777777	0600407		a.out SunOS SPARC
>0	byte		&0x80		dynamically linked executable
>0	byte		^0x80		executable
>16	belong		>0		not stripped

0	belong&077777777	0400413		a.out SunOS mc68020 demand paged
>0	byte		&0x80
>>20	belong		<4096		shared library
>>20	belong		=4096		dynamically linked executable
>>20	belong		>4096		dynamically linked executable
>0	byte		^0x80		executable
>16	belong		>0		not stripped

0	belong&077777777	0400410		a.out SunOS mc68020 pure
>0	byte		&0x80		dynamically linked executable
>0	byte		^0x80		executable
>16	belong		>0		not stripped

0	belong&077777777	0400407		a.out SunOS mc68020
>0	byte		&0x80		dynamically linked executable
>0	byte		^0x80		executable
>16	belong		>0		not stripped

0	belong&077777777	0200413		a.out SunOS mc68010 demand paged
>0	byte		&0x80
>>20	belong		<4096		shared library
>>20	belong		=4096		dynamically linked executable
>>20	belong		>4096		dynamically linked executable
>0	byte		^0x80		executable
>16	belong		>0		not stripped

0	belong&077777777	0200410		a.out SunOS mc68010 pure
>0	byte		&0x80		dynamically linked executable
>0	byte		^0x80		executable
>16	belong		>0		not stripped

0	belong&077777777	0200407		a.out SunOS mc68010
>0	byte		&0x80		dynamically linked executable
>0	byte		^0x80		executable
>16	belong		>0		not stripped

#
# Core files.  "SPARC 4.x BCP" means "core file from a SunOS 4.x SPARC
# binary executed in compatibility mode under SunOS 5.x".
#
0	belong		0x080456	SunOS core file
>4	belong		432		(SPARC)
>>132	string		>\0		from '%s'
>>116	belong		=3		(quit)
>>116	belong		=4		(illegal instruction)
>>116	belong		=5		(trace trap)
>>116	belong		=6		(abort)
>>116	belong		=7		(emulator trap)
>>116	belong		=8		(arithmetic exception)
>>116	belong		=9		(kill)
>>116	belong		=10		(bus error)
>>116	belong		=11		(segmentation violation)
>>116	belong		=12		(bad argument to system call)
>>116	belong		=29		(resource lost)
>>120	belong		x		(T=%dK,
>>124	belong		x		D=%dK,
>>128	belong		x		S=%dK)
>4	belong		826		(68K)
>>128	string		>\0		from '%s'
>4	belong		456		(SPARC 4.x BCP)
>>152	string		>\0		from '%s'
# Sun SunPC
0	long		0xfa33c08e	SunPC 4.0 Hard Disk
0	string		#SUNPC_CONFIG	SunPC 4.0 Properties Values
# Sun snoop (see RFC 1761, which describes the capture file format,
# RFC 3827, which describes some additional datalink types, and
# https://www.iana.org/assignments/snoop-datalink-types/snoop-datalink-types.xml,
# which is the IANA registry of Snoop datalink types)
#
0	string		snoop		Snoop capture file
>8	belong		>0		- version %d
>12	belong		0		(IEEE 802.3)
>12	belong		1		(IEEE 802.4)
>12	belong		2		(IEEE 802.5)
>12	belong		3		(IEEE 802.6)
>12	belong		4		(Ethernet)
>12	belong		5		(HDLC)
>12	belong		6		(Character synchronous)
>12	belong		7		(IBM channel-to-channel adapter)
>12	belong		8		(FDDI)
>12	belong		9		(Other)
>12	belong		10		(type %d)
>12	belong		11		(type %d)
>12	belong		12		(type %d)
>12	belong		13		(type %d)
>12	belong		14		(type %d)
>12	belong		15		(type %d)
>12	belong		16		(Fibre Channel)
>12	belong		17		(ATM)
>12	belong		18		(ATM Classical IP)
>12	belong		19		(type %d)
>12	belong		20		(type %d)
>12	belong		21		(type %d)
>12	belong		22		(type %d)
>12	belong		23		(type %d)
>12	belong		24		(type %d)
>12	belong		25		(type %d)
>12	belong		26		(IP over Infiniband)
>12	belong		>26		(type %d)

#---------------------------------------------------------------------------
# The following entries have been tested by Duncan Laurie <duncan@sun.com> (a
# lead Sun/Cobalt developer) who agrees that they are good and worthy of
# inclusion.

# Boot ROM images for Sun/Cobalt Linux server appliances
0       string  Cobalt\ Networks\ Inc.\nFirmware\ v     Paged COBALT boot rom
>38     string x        V%.4s

# New format for Sun/Cobalt boot ROMs is annoying, it stores the version code
# at the very end where file(1) can't get it.
0       string CRfs     COBALT boot rom data (Flat boot rom or file system)
